|  |  |
| --- | --- |
| **Setup Use Case** | |
| **Actors** | Operator |
| **Preconditions** | ChronoTimer is off |
| **Normal Course** | 1. Operator turns the ChronoTimer on.    1. ChronoTimer sets current time to internal clock. |
| **Alternate Courses** | Operator may also turn ChronoTimer printer on at this stage. |
| **Exception Courses** | If the ChronoTimer is unable to power on, operator should check power connection. |
| **Post-conditions** | ChronoTimer is on with the current time set. |
| **Frequency of Use** | High |
| **Assumptions** | - |